LEGO instructions – for printing/cutting

1. You are **the leader** of the group. You must ensure there is only one single construction created by the group.
2. You are **the only person** who is allowed to build (assemble bricks) in the first (1st) and seventh (7th) brick layers in the construction – do not allow others to build in these layers
3. You are **the only person** who is allowed to build (assemble bricks) in the third (3rd) and eighth (8th) layer of bricks in the construction ­– do not allow others to build in these layers
4. You are **the only person** who is allowed to build (assemble bricks) in the second (2nd) and sixth (6th) layer of bricks in the construction ­– do not allow others to build in these layers
5. You are **the only person** who is allowed to build (assemble bricks) in the fourth (4th) and fifth (5th) layer of bricks in the construction ­– do not allow others to build in these layers
6. You must ensure there is at least one gap, or a ‘missing block’ in the second, fourth and sixth (2nd, 4th and 6th) layers.
7. You must ensure that the bricks in the first (1st) layer of the construction change in colours (no 2 bricks of the same colour may touch each other) and that the fourth (4th) layer includes bricks of different sizes (different block lengths)
8. You must ensure that the construction is a maximum 8 brick layers high, and the first layer includes bricks of different sizes (different block lengths). You must make sure no two blocks of the same colour touch each other in the 6th layer.
9. You must ensure that the third and fourth (3rd and 4th ) layer of bricks in the construction only consist of yellow bricks, make sure that at least four blocks in the eighth layer (and 8th) are green.
10. You must ensure that 2nd and 5th layer in the construction only consists of red bricks, the 6th layer must have at least three red bricks
11. You must ensure that 2nd and 6th layer of bricks in the construction consist of exactly 8 bricks and that these layers (2 and 6) have at least one block at ‘right angles’ to the rest of the layer
12. You must ensure that the 2nd, 4th, 6th and 8th layers are not all the same colour – but also that the last bricks (the end bricks) are always the same colour on every layer (if the colours are mixed)
13. You must ensure that a maximum of 8 bricks are used in the 3rd and 5th brick layer in the construction, and that these layers (3 and 5) have at least one block at ‘right angles’ to the rest of the layer